**Project: Solar Orbiter SWA**

**Author:** **Gethyn Lewis**

**TITLE: SWA Instrument Post Covid Commission Plan**

**Document Number: SO-SWA-MSSL-PL 0XX Issue 15**

**Date:**

**CHANGE RECORD**

|  |  |  |  |
| --- | --- | --- | --- |
| **ISSUE** | **DATE** | **PAGES CHANGED** | **COMMENTS** |
| 1 |  |  | All new |
| 2 |  |  |  |
| 3 |  |  |  |
| 4 |  |  |  |
| 5 |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

**CONTENTS**

1 Introduction 5

2 Reference Documents 5

3 Acronym and Abbreviation List 6

4 General requirements 7

4.1 Spacecraft Location and Plasma Environment 7

4.2 Required Configuration of the Spacecraft 7

4.3 Spacecraft Pointing 7

4.4 Spacecraft-generated Gases 7

4.5 Telemetry 7

4.6 Required Configuration of other Instruments 7

4.7 Inter-Experiment Links - Service 20 7

4.8 Verification process during commissioning 8

Performance Verification 8

Spacecraft EGSE Real-time Housekeeping Parameters 8

Real-time SWA Housekeeping Parameters 8

Real-time SWA Science Data 8

4.9 Order of commissioning of the DPU and SWA sensors 8

5 15th April. SWA-4 (IA-4) Day 2 10

5.1 PAS Power On 10

5.2 PAS Ramp up main HV 12

5.3 PAS Detector commission 15

5.4 PAS Normal science check 25

5.5 MTL PDOR\_SSWA\_SWA\_MTL\_15Apr\_00002.SOL 27

6 16th April. SWA-5 (IA-5) 31

6.1 MTL PDOR\_SSWA\_SWA\_MTL\_16Apr\_00002.SOL 31

6.2 EAS 1&2 Eng Mode 6 44

6.3 EAS 2 MCP commission 45

6.4 EAS 2 Zero Sweeps 48

6.5 EAS2 Flight deflectors 49

6.6 EAS2 POST MCP commission 50

6.7 EAS 2 Flight Sweeps 51

6.8 EAS2 Start Normal Mode 53

6.9 EAS1 MCP commission 53

6.10 EAS1 Zero Sweeps 55

6.11 EAS1 Flight Sweeps 57

6.12 EAS1 Flight deflectors 58

6.13 EAS1 POST MCP commission 59

6.14 EAS1 Flight Voltage Offsets 59

6.15 EAS1 Start Normal Mode 60

6.16 EAS 2 Engineering modes 62

6.17 EAS 2 Reset Sweeps 68

6.18 EAS 1 Engineering modes 72

6.19 EAS 1 Reset Sweeps 78

6.20 EAS Flight Like Gain Test 81

6.21 EAS Reset MCP 84

6.22 EAS Start Normal Mode 85

6.23 EAS 1&2 Eng Mode 7 86

6.24 EAS FDIR Commission 87

6.25 EAS Reset MCP 89

6.26 EAS Start Normal Mode 90

6.27 EAS Configure heater 91

6.28 MTL PDOR\_SSWA\_SWA\_MTL\_16Apr\_00001.SOL 92

7 22nd April. SWA-6 (IA-6) 95

7.1 MTL PDOR\_SSWA\_SWA\_MTL\_22Apr\_00001.SOL 95

7.2 SWA Normal mode 96

7.3 PAS Calibration mode 103

7.4 SWA Burst mode 104

7.5 SWA Cadence test 106

8 SWA Commission conclusion 114

9 Appendices 115

9.1 Emergency Contingency Plans 115

# Introduction

The primary objective of this document is to describe the in-flight commissioning plan of the SWA flight instrument. The proposed tests will demonstrate that the performance of the instrument meets the operational requirements. The aim is to define activities with an emphasis on performing tests that require real time contact with the spacecraft.

# Reference Documents

The documents listed below form a part of this document, to the extent specified and described herein.

|  |  |  |
| --- | --- | --- |
| Ref. | No | Title |
| NR1 | SOL-EST-IF-0050 | Solar Orbiter Experiment Interface Document Part A |
| NR2 | SOL-EST-RS-1937 | Solar Orbiter Product Assurance Requirements for Instruments |
| NR3 | SO-SWA-MSSL-SP-006 | SWA Instrument Scientific Requirements Report |
| NR4 | SO-SWA-MSSL-PL-006 | SWA Product Assurance Plan |
| NR5 | MSSL-SO-SWA-EID-B | SWA EID-B |
| NR6 | SO-SWA-LPP-LP-039\_MCP Acceptance Test | LPP MCP Acceptance and characterisation Plan |
| NR7 | SO-SWA-LPP-RP-078\_1\_1-MCP\_test\_report\_PartI | MCP detector characterisation test report |
| NR8 | SO-SWA-LPP-RP-092 EAS Det FM1 Test Report rev 1-4.pdf | LPP detector sub-system test report FM1 |
| NR9 | SO-SWA-LPP-RP-093 EAS Det FM2 Test Report rev 1-2.pdf | LPP detector sub-system test report FM2 |
| NR10 | SO-SWA-MSSL-SP-012\_EAS-DPU\_Interface\_Specification\_Issue\_2.pdf | EAS-DPU Interface Specification |
| NR11 | SO-SWA-MSSL-PL-013 | SWA EAS Calibration Plan |
| NR12 | SO-SWA-MSSL-UM-002 | SWA Instrument User manual |

# Acronym and Abbreviation List

|  |  |
| --- | --- |
| **Abbreviation** | **Meaning** |
| PDOR | Payload Direct Operations Request |
| MDOR | Memory Direct Operations Request |
| IA-FCP | Instrument (SWA) – Flight Control Procedure |
| TC | TeleCommand |
| IIC | Inter Instrument Check |
|  |  |
|  |  |

# General requirements

## Spacecraft Location and Plasma Environment

To be included

## Required Configuration of the Spacecraft

There is no particular spacecraft configuration required during SWA commission.

## Spacecraft Pointing

There is no designated pointing required during the SWA commission phase.

## Spacecraft-generated Gases

SWA commissioning, particularly involving high voltages, should not begin until sufficient time has elapsed for spacecraft outgassing to be essentially complete. It has been estimated that at least 20 days are required after launch, following assessment of data from TQCM.

No thruster firing should occur during SWA commissioning, and a sufficient time should be allowed between any thruster firing and the start of commissioning.

## Telemetry

A telemetry requirement of xxx will be required for SWA commissioning

## Required Configuration of other Instruments

It is accepted by SWA that some other instruments are powered on during the SWA commission. However if SWA feel that the other instruments are causing interference to SWA commission, then SWA will request that those instruments be powered down. It is also expected that no other instrument commanding will take place during SWA commission periods.

## Inter-Experiment Links - Service 20

The IEL inputs to SWA are from

* MAG
* RPW

Until completion of commissioning of each sensor, IEL inputs will be disabled at the DPU.

## Verification process during commissioning

### Performance Verification

Following each command in the commissioning sequence the experimenter will either confirm that the command was executed as expected or recommend that a contingency plan is executed.

### Spacecraft EGSE Real-time Housekeeping Parameters

Checking of the housekeeping parameters will be performed using the spacecraft EGSE. Visual checking of the real time housekeeping by a SWA team member viewing the ESOC video display.  **Unless otherwise stated, each command in the commissioning sequences given should be followed by inspection of the housekeeping by an SWA team member before the next command in the sequence is sent.**

### Real-time SWA Housekeeping Parameters

Visual checking of the near-real time housekeeping data by an SWA team member viewing the SWA EGSE display. Data will be acquired via tbd mechanism. The EGSE provides a range of graphical displays for the interpretation of the housekeeping and science data and will have limit checking similar to that used for ground testing. Specific parameters which will be checked in this way are listed in the detailed procedures in this document.

### Real-time SWA Science Data

Real-time assessment of science data from the SWA sensors will be required during commissioning. Interpretation and visualisation of the data will use SWA provided EGSE, both for engineering and science assessments.

## Order of commissioning of the DPU and SWA sensors

The basic order of commissioning of the different SWA units is as follows:

* DPU
* HIS
* PAS
* EAS
* All SWA

The outline plan for SWA commission is provided in the MOC NECP Timeline plan. Currently this is illustrated in Table 4.1

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **NECP Phase** | **NECP number** | **Date** | **Day** | **Start Time** | **End Time** | **Duration** | **One Way Light Time (Seconds)** | **Comments** |
| SWA-3 | IA-3 | 22 Apr | Wed | 07:20 | 15:20 | 08:00 | 105-117 | HIS |
| SWA-3 | IA-3 | 24 Apr | Fri | 07:20 | 15:20 | 08:00 | 105-117 | HIS |
| SWA-3 | IA-3 | 28 Apr | Tue | 09:27 | 17:27 | 08:00 | 123-117 | HIS |
| SWA-3 | IA-5 | 29 Apr | Wed | 09:21 | 17:27 | 08:06 | 123-117 | HIS |
| SWA-5 | IA-5 | 30 Apr | Thu | 09:15 | 17:15 | 08:00 | 123-117 | EAS |
| SWA-5 |  | 05-May | Tue | 14:48 | 19:06 | 04:18 | 146-147 |  |
| SWA-6 |  | 06-May | Wed | 12:42 | 19:00 | 06:18 | 146-147 | SWA |
| SWA-6 |  | 07-May | Thu | 20:00 | 05:00 | 09:00 | 146-147 | SWA |
| SWA-6 |  | 08-May | Fri | 06:22 | 14:22 | 08:00 | 146-147 | SWA |
| SWA-6 |  | 11-May | Mon | 06:07 | 14:07 | 08:00 | 177-203 | SWA |
| IIC |  | 20-May | Wed | 15:00 | 18:00 | 03:00 | 215-248 | IIC |
| EMC |  | 02-Jun | Tue | 01:00 | 10:17 | 09:17 | 319-362 | EMC |

Table 4.1 MOC Timeline for each SWA commission phase (version 5.6). All times are in UTC.

# 22nd April. SWA-3 (IA-3) HIS

|  |  |  |  |
| --- | --- | --- | --- |
| **Start Time** | **End Time** | **Description** | **PDOR** |
| 07:20 |  | Pass Starts |  |
| 07:20 | 07:30 | Load commands on the MTL to ramp down the PA-HVPS, Turn OFF SWA-HIS, and Turn OFF SWA-DPU | PDOR\_SSWA\_HIS\_10\_PA\_RAMP\_DOWN\_MTL\_20200422\_00001  PDOR\_SSWA\_HIS\_2\_DPU\_HIS\_OFF\_MTL\_20200422\_00001 |
| 07:30 | 07:40 | Turn on SWA-DPU and SWA-HIS | PDOR\_SSWA\_HIS\_1\_DPU\_HIS\_ON\_00001 |
| 07:40 | 08:06 | Ramp PA-HVPS up to 7.5kV | PDOR\_SSWA\_HIS\_7\_PA\_RAMP\_UP\_7500\_00001 |
| 08:06 | 10:58 | PA-HPVS commissioning to 16kV | PDOR\_SSWA\_HIS\_12\_PA\_DAY\_1\_00002 |
| 10:58 | 11:13 | Load MCP ramp down onto MTL and load MTL PDORs for 24-April pass | PDOR\_SSWA\_HIS\_5\_MCP\_RAMP\_DOWN\_DISABLE\_MTL\_20200422\_00001  PDOR\_SSWA\_HIS\_1\_DPU\_HIS\_ON\_MTL\_20200424\_00001  PDOR\_SSWA\_HIS\_8\_PA\_RAMP\_UP\_14000\_00001\_MTL\_20200424  PDOR\_SSWA\_HIS\_10\_PA\_RAMP\_DOWN\_MTL\_20200424\_00001  PDOR\_SSWA\_HIS\_2\_DPU\_HIS\_OFF\_MTL\_20200424\_00001 |
| 11:13 | 12:03 | Enable MCPs and ramp to 1.7kV (automatic once stated) | PDOR\_SSWA\_HIS\_3\_MCP\_RAMP\_UP\_1700\_00002 |
| 12:03 | 14:33 | MCP commissioning | PDOR\_SSWA\_HIS\_6\_MCP\_STEP\_UP\_1750\_2130\_00001 |
| 14:33 | 15:20 | Margin |  |
| 15:20 |  | Pass Ends |  |
| 15:20 | 19:30 | SSD Threshold Test (start interactive or this doesn’t happen on this date) | PDOR\_SSWA\_HIS\_15\_SSD\_NOISE\_TEST\_00002 |
| 19:30 | 20:15 | Ramp down MCPs from MTL (nominal plan) | Loaded at 10:58 (HIS\_5\_MCP\_RAMP\_DOWN\_DISABLE\_MTL\_20200422) |
| 20:15 | 21:15 | SAFETY Ramp down PA-HVPS from MTL (will nominally fail) | Loaded at 07:20 (HIS\_10\_PA\_RAMP\_DOWN\_MTL\_20200422) |
| 21:15 | 21:27 | Power off SWA-HIS from MTL (nominal plan) | Loaded at 07:20 (HIS\_2\_DPU\_HIS\_OFF\_MTL\_20200422) |
| 21:27 | 21:30 | Power off SWA-DPU from MTL (nominal plan) | Loaded at 07:20 (HIS\_2\_DPU\_HIS\_OFF\_MTL\_20200422) |
| 22:00 |  | WOL Starts |  |

# 24th April. SWA-3 (IA-3) HIS

|  |  |  |  |
| --- | --- | --- | --- |
| **Start Time** | **End Time** | **Description** | **PDOR** |
| 06:08 | 06:18 | Power on SWA-DPU and SWA-HIS from MTL | Loaded 22-Apr at 10:58 (HIS\_1\_DPU\_HIS\_ON\_MTL\_20200424\_00001) |
| 06:18 | 07:00 | Ramp PA-HVPS to 14kV from MTL | Loaded 22-Apr at 10:58 (HIS\_8\_PA\_RAMP\_UP\_14000\_00001\_MTL\_20200424) |
| 07:00 | 07:20 | Margin |  |
| 07:20 |  | Pass Starts |  |
| 07:20 | 14:56 | PA-HVPS commissioning to 22.5kV | PDOR\_SSWA\_HIS\_13\_PA\_DAY\_2\_00002 |
| 14:56 | 15:11 | Load PDORs for 28-April to MTL | PDOR\_SSWA\_HIS\_1\_DPU\_HIS\_ON\_MTL\_20200428\_00001  PDOR\_SSWA\_HIS\_9\_PA\_RAMP\_UP\_20500\_00001\_MTL\_20200428  PDOR\_SSWA\_HIS\_10\_PA\_RAMP\_DOWN\_MTL\_20200428\_00001  PDOR\_SSWA\_HIS\_2\_DPU\_HIS\_OFF\_MTL\_20200428\_00001 |
| 15:11 | 15:20 | Margin |  |
| 15:20 |  | Pass Ends |  |
| 15:20 | 16:20 | SAFETY Ramp down PA-HVPS from MTL (will nominally fail) | Loaded 22-Apr at 10:58 (HIS\_10\_PA\_RAMP\_DOWN\_MTL\_20200424) |
| 16:20 | 16:32 | Power off SWA-HIS from MTL (nominal plan) | Loaded 22-Apr at 10:58 (HIS\_2\_DPU\_HIS\_OFF\_MTL\_20200424) |
| 16:32 | 16:35 | Power off SWA-DPU from MTL (nominal plan) | Loaded 22-Apr at 10:58 (HIS\_2\_DPU\_HIS\_OFF\_MTL\_20200424) |
| 22:00 |  | WOL Starts |  |

# 28th April. SWA-3 (IA-3) HIS

|  |  |  |  |
| --- | --- | --- | --- |
| **Start Time** | **End Time** | **Description** | **PDOR** |
| 07:42 | 07:52 | Power on SWA-DPU and SWA-HIS from MTL | Loaded 24-Apr at 14:56 (HIS\_1\_DPU\_HIS\_ON\_MTL\_20200428) |
| 07:52 | 08:57 | Ramp PA-HVPS to 20.5kV from MTL | Loaded 24-Apr at 14:56 (HIS\_9\_PA\_RAMP\_UP\_20500\_00001\_MTL\_20200428) |
| 08:57 | 09:27 | Margin |  |
| 09:27 |  | Pass Starts |  |
| 09:27 | 17:14 | PA-HVPS commissioning to 26kV | PDOR\_SSWA\_HIS\_14\_PA\_DAY\_3\_00002 |
| 17:14 | 17:27 | Margin |  |
| 17:27 |  | Pass Ends |  |
| 17:27 | 18:27 | Post-Pass Margin |  |
| 18:27 | 19:27 | SAFETY Ramp down PA-HVPS from MTL (will nominally fail) | Loaded 4-24 at 14:56 (HIS\_10\_PA\_RAMP\_DOWN\_MTL\_20200428) |
| 19:27 | 19:39 | Power off SWA-HIS from MTL (nominal plan) | Loaded 4-24 at 14:56 (HIS\_2\_DPU\_HIS\_OFF\_MTL\_20200428) |
| 19:39 | 19:42 | Power off SWA-DPU from MTL (nominal plan) | Loaded 4-24 at 14:56 (HIS\_2\_DPU\_HIS\_OFF\_MTL\_20200428) |

# 29th April. SWA-3 (IA-3) EAS & PAS

## MTL PDOR\_SSWA\_SWA\_MTL\_29Apr\_00001.SOL

|  |  |  |  |
| --- | --- | --- | --- |
| **Step N°** | **Commanding Flow** | **FCP ID or PDOR title & contents** | **Comments** |
|  | START DPU  UniqueID = SSWAEAStest01 | AIAF011A | 2020-120T09:20:00.000Z |
|  | DPU TO OPS  UniqueID = SSWAEAStest02 | AIAF030A | 2020-120T09:25:00.000Z |
|  | DISABLE EAS1 FDIR  UniqueID = SSWAEAStest03 | ZIA58064 PIA60452 position=1 = 12  PIA60449 position=2 = EAS1SPWHB\_MI  PIA60449 position=3 = E1\_3V3\_MI  PIA60449 position=4 = E1\_1V5\_MI  PIA60449 position=5 = E1OPTEMPMON  PIA60449 position=6 = E1HVOUTVMON  PIA60449 position=7 = E1MCPVMON  PIA60449 position=8 = E1GRIDVMON  PIA60449 position=9 = E110VAPOSVMON  PIA60449 position=10 = E128VPOSVMON  PIA60449 position=11 = E1HVGENTHERMON  PIA60449 position=12 = E1HVMODTHERMON  PIA60449 position=13 = EAS1MISSACK\_MI | 2020-120T09:30:00.000Z |
|  | DISABLE EAS2 FDIR  UniqueID = SSWAEAStest04 | ZIA58064 PIA60452 position=1 = 12  PIA60449 position=2 = EAS2SPWHB\_MI  PIA60449 position=3 = E2\_3V3\_MI  PIA60449 position=4 = E2\_1V5\_MI  PIA60449 position=5 = E2OPTEMPMON  PIA60449 position=6 = E2HVOUTVMON  PIA60449 position=7 = E2MCPVMON  PIA60449 position=8 = E2GRIDVMON  PIA60449 position=9 = E210VAPOSVMON  PIA60449 position=10 = E228VPOSVMON  PIA60449 position=11 = E2HVGENTHERMON  PIA60449 position=12 = E2HVMODTHERMON  PIA60449 position=13 = EAS2MISSACK\_MI | 2020-120T09:30:10.000Z |
|  | ENABLE HK  UniqueID = SSWAEAStest05 | ZIA58050 PIA58050 position=1 = EAS1\_SENS\_HK | 2020-120T09:30:20.000Z |
|  | POWER ON EAS1  UniqueID = SSWAEAStest06 | ZIA58760 | 2020-120T09:30:30.000Z |
|  | RUN POST MACRO  UniqueID = SSWAEAStest07 | ZIA58934 PIA60739 position=1 = POST | 2020-120T09:31:00.000Z |
|  | RUN IDLE MACRO  UniqueID = SSWAEAStest08 | ZIA58753 | 2020-120T09:31:30.000Z |
|  | REQUEST HK  UniqueID = SSWAEAStest09 | ZIA58782 | 2020-120T09:32:00.000Z |
|  | RUN MACRO  UniqueID = SSWAEAStest10 | ZIA58758 | 2020-120T09:32:10.000Z |
|  | ENABLE HK  UniqueID = SSWAEAStest11 | ZIA58050 PIA58050 position=1 = EAS2\_SENS\_HK | 2020-120T09:32:20.000Z |
|  | POWER ON EAS2  UniqueID = SSWAEAStest12 | ZIA58808 | 2020-120T09:32:30.000Z |
|  | RUN POST MACRO  UniqueID = SSWAEAStest13 | ZIA58936 PIA60740 position=1 = POST | 2020-120T09:33:00.000Z |
|  | RUN IDLE MACRO  UniqueID = SSWAEAStest14 | ZIA58801 | 2020-120T09:33:30.000Z |
|  | REQUEST HK  UniqueID = SSWAEAStest15 | ZIA58830 | 2020-120T09:33:40.000Z |
|  | RUN MACRO  UniqueID = SSWAEAStest16 | ZIA58806 | 2020-120T09:34:00.000Z |
|  | EAS1 MCR  UniqueID = SSWAEAStest17 | ZIA58776 PIA60423 position=1 = 00  PIA60424 position=2 = 40  PIA60425 position=3 = 60 | 2020-120T09:35:00.000Z |
|  | EAS1 HEATER ON  UniqueID = SSWAEAStest18 | ZIA58757 PIA60773 position=1 = 00  PIA60774 position=2 = 00  PIA60775 position=3 = E8 | 2020-120T09:35:10.000Z |
|  | EAS2 MCR  UniqueID = SSWAEAStest19 | ZIA58824 PIA60423 position=1 = 00  PIA60424 position=2 = 40  PIA60425 position=3 = 60 | 2020-120T09:35:20.000Z |
|  | EAS2 HEATER ON  UniqueID = SSWAEAStest20 | ZIA58805 PIA60773 position=1 = 00  PIA60774 position=2 = 00  PIA60775 position=3 = E8 | 2020-120T09:35:30.000Z |
|  | SET CADENCE  UniqueID = SSWAEAStest21 | ZIA58728 PIA60096 position=1 = NOMINAL\_CADENCE  PIA60097 position=2 = NOMINAL\_CADENCE  PIA60099 position=3 = NOMINAL\_CADENCE  PIA60098 position=4 = NOMINAL\_CADENCE | 2020-120T09:35:40.000Z |
|  | ZERO EAS1 DEFLECTORS  UniqueID = SSWAEAStest22 | ZIA58765 PIA60474 position=1 = 00  PIA60475 position=2 = 00  PIA60578 position=3 = 00  PIA60589 position=4 = 00  PLUS 96 BYTES | 2020-120T09:35:41.000Z |
|  | ZERO EAS2 DEFLECTORS  UniqueID = SSWAEAStest23 | ZIA58813 PIA60474 position=1 = 00  PIA60475 position=2 = 00  PIA60578 position=3 = 00  PIA60589 position=4 = 00  PLUS 96 BYTES | 2020-120T09:35:50.000Z |
|  | START EAS2 ENG MODE 5  UniqueID = SSWAEAStest24 | ZIA58839 PIA60454 position=1 = FF  PIA60455 position=2 = FF  PIA60040 position=3 = 724  PIA60039 position=4 = 477  PIA60041 position=5 = 76  PIA60106 position=6 = 0  PIA60171 position=7 = A  PIA60165 position=8 = 2 | 2020-120T09:36:00.000Z |
|  | EAS2 THRESHOLDS  UniqueID = SSWAEAStest25 | ZIA58845 PIA60174 position=1 = 4C80  PIA60185 position=2 = 4C81  PIA60196 position=3 = 4C82  PIA60200 position=4 = 4C83  PIA60201 position=5 = 4C84  PIA60202 position=6 = 4C85  PIA60203 position=7 = 4C86  PIA60204 position=8 = 4C87  PIA60205 position=9 = 4C88  PIA60175 position=10 = 4C89  PIA60176 position=11 = 4C8A  PIA60177 position=12 = 4C8B  PIA60178 position=13 = 4C8C  PIA60179 position=14 = 4C8D  PIA60180 position=15 = 4C8E  PIA60181 position=16 = 4C8F  PIA60182 position=17 = 4C80  PIA60183 position=18 = 4C81  PIA60184 position=19 = 4C82  PIA60186 position=20 = 4C83  PIA60187 position=21 = 4C84  PIA60188 position=22 = 4C85  PIA60189 position=23 = 4C86  PIA60190 position=24 = 4C87  PIA60191 position=25 = 4C88  PIA60192 position=26 = 4C89  PIA60193 position=27 = 4C8A  PIA60194 position=28 = 4C8B  PIA60195 position=29 = 4C8C  PIA60197 position=30 = 4C8D  PIA60198 position=31 = 4C8E  PIA60199 position=32 = 4C8F | 2020-120T09:45:40.000Z |
|  | START EAS2 ENG MODE 6  UniqueID = SSWAEAStest26 | ZIA58840 PIA60457 position=1 = FF  PIA60458 position=2 = 32  PIA60459 position=3 = 28  PIA60106 position=4 = 0  PIA60171 position=5 = A  PIA60165 position=6 = 10 | 2020-120T09:46:00.000Z |
|  | SET THE EAS2 HEM RATIO  UniqueID = SSWAEAStest27 | ZIA58814 PIA60469 position=1 = DE  PIA60470 position=2 = B8  PIA60471 position=3 = 51 | 2020-120T09:56:00.000Z |
|  | SET EAS2 HEM VOLTAGE TO 800  UniqueID = SSWAEAStest28 | ZIA58815 PIA60441 position=1 = 67  PIA60442 position=2 = 18  PIA60443 position=3 = A0 | 2020-120T09:56:10.000Z |
|  | REBUILD HEM TABLE  UniqueID = SSWAEAStest29 | ZIA58819 PIA60031 position=1 = MBOX3  PIA60446 position=2 = 0  PIA60447 position=3 = 0  PIA60448 position=4 = 1 | 2020-120T09:56:20.000Z |
|  | EAS2 FLIGHT VOLT OFFSETS  UniqueID = SSWAEAStest30 | ZIA58817 PIA60411 position=1 = 01  PIA60412 position=2 = E0  PIA60415 position=3 = 70  PIA60416 position=4 = 01  PIA60417 position=5 = A7  PIA60418 position=6 = D0  PIA60419 position=7 = 01  PIA60420 position=8 = BD  PIA60421 position=9 = 70  PIA60422 position=10 = 01  PIA60413 position=11 = B4  PIA60414 position=12 = 40 | 2020-120T09:56:30.000Z |
|  | START EAS2 ENG MODE 5  UniqueID = SSWAEAStest31 | ZIA58839 PIA60454 position=1 = FF  PIA60455 position=2 = FF  PIA60040 position=3 = 724  PIA60039 position=4 = 477  PIA60041 position=5 = 76  PIA60106 position=6 = 0  PIA60171 position=7 = A  PIA60165 position=8 = 2 | 2020-120T09:57:00.000Z |
|  | EAS2 MCP TO ????  UniqueID = SSWAEAStest32 | ZIA58832 PIA60218 position=1 = 0 | 2020-120T10:09:30.000Z |
|  | EAS2 THRESHOLDS  UniqueID = SSWAEAStest33 | ZIA58845 PIA60174 position=1 = 4C80  PIA60185 position=2 = 4C81  PIA60196 position=3 = 4C82  PIA60200 position=4 = 4C83  PIA60201 position=5 = 4C84  PIA60202 position=6 = 4C85  PIA60203 position=7 = 4C86  PIA60204 position=8 = 4C87  PIA60205 position=9 = 4C88  PIA60175 position=10 = 4C89  PIA60176 position=11 = 4C8A  PIA60177 position=12 = 4C8B  PIA60178 position=13 = 4C8C  PIA60179 position=14 = 4C8D  PIA60180 position=15 = 4C8E  PIA60181 position=16 = 4C8F  PIA60182 position=17 = 4C80  PIA60183 position=18 = 4C81  PIA60184 position=19 = 4C82  PIA60186 position=20 = 4C83  PIA60187 position=21 = 4C84  PIA60188 position=22 = 4C85  PIA60189 position=23 = 4C86  PIA60190 position=24 = 4C87  PIA60191 position=25 = 4C88  PIA60192 position=26 = 4C89  PIA60193 position=27 = 4C8A  PIA60194 position=28 = 4C8B  PIA60195 position=29 = 4C8C  PIA60197 position=30 = 4C8D  PIA60198 position=31 = 4C8E  PIA60199 position=32 = 4C8F | 2020-120T10:09:40.000Z |
|  | START EAS2 ENG MODE 6  UniqueID = SSWAEAStest34 | ZIA58840 PIA60457 position=1 = FF  PIA60458 position=2 = 32  PIA60459 position=3 = 28  PIA60106 position=4 = 0  PIA60171 position=5 = A  PIA60165 position=6 = 10 | 2020-120T10:10:00.000Z |
|  | START EAS2 ENG MODE 3  UniqueID = SSWAEAStest35 | ZIA58837 PIA60101 position=1 = 869  PIA60100 position=2 = A53  PIA60102 position=3 = 1E  PIA60437 position=4 = A  PIA60444 position=5 = 1  PIA60165 position=6 = 40  PIA60760 position=7 = 0D  PIA60761 position=8 = 8  PIA60762 position=9 = SWEEP\_MACRO | 2020-120T10:15:00.000Z |
|  | EAS2 MCP TO ???  UniqueID = SSWAEAStest36 | ZIA58832 PIA60218 position=1 = 0 | 2020-120T10:19:50.000Z |
|  | START EAS2 ENG MODE 4  UniqueID = SSWAEAStest37 | ZIA58838 PIA60104 position=1 = 6BC  PIA60103 position=2 = 4BE  PIA60105 position=3 = 1E  PIA60106 position=4 = A94  PIA60165 position=5 = A  PIA60851 position=6 = 20  PIA60760 position=7 = 0D  PIA60761 position=8 = 8 | 2020-120T10:20:00.000Z |
|  | SET EAS2 HEM VOLTAGE TO 0  UniqueID = SSWAEAStest38 | ZIA58815 PIA60441 position=1 = 0  PIA60442 position=2 = 0  PIA60443 position=3 = 0 | 2020-120T10:30:00.000Z |
|  | REBUILD HEM TABLE  UniqueID = SSWAEAStest39 | ZIA58819 PIA60031 position=1 = MBOX3  PIA60446 position=2 = 0  PIA60447 position=3 = 0  PIA60448 position=4 = 1 | 2020-120T10:30:20.000Z |
|  | ZERO EAS2 FLIGHT VOLT OFFSETS  UniqueID = SSWAEAStest40 | ZIA58817 PIA60411 position=1 = 0  PIA60412 position=2 = 0  PIA60415 position=3 = 0  PIA60416 position=4 = 0  PIA60417 position=5 = 0  PIA60418 position=6 = 0  PIA60419 position=7 = 0  PIA60420 position=8 = 0  PIA60421 position=9 = 0  PIA60422 position=10 = 0  PIA60413 position=11 = 0  PIA60414 position=12 = 0 | 2020-120T10:30:30.000Z |
|  | START EAS2 ENG MODE 4  UniqueID = SSWAEAStest41 | ZIA58838 PIA60104 position=1 = 6BC  PIA60103 position=2 = 4BE  PIA60105 position=3 = 1E  PIA60106 position=4 = A94  PIA60165 position=5 = A  PIA60851 position=6 = 20  PIA60760 position=7 = 0D  PIA60761 position=8 = 8 | 2020-120T10:31:00.000Z |
|  | START EAS2 ENG MODE 7  UniqueID = SSWAEAStest42 | ZIA58841 | 2020-120T10:40:00.000Z |
|  | SET EAS2 HEM VOLTAGE TO 800  UniqueID = SSWAEAStest43 | ZIA58815 PIA60441 position=1 = 67  PIA60442 position=2 = 18  PIA60443 position=3 = A0 | 2020-120T10:45:00.000Z |
|  | REBUILD HEM TABLE  UniqueID = SSWAEAStest44 | ZIA58819 PIA60031 position=1 = MBOX3  PIA60446 position=2 = 0  PIA60447 position=3 = 0  PIA60448 position=4 = 1 | 2020-120T10:45:20.000Z |
|  | SET EAS2 FLIGHT VOLT OFFSETS  UniqueID = SSWAEAStest45 | ZIA58817 PIA60411 position=1 = 01  PIA60412 position=2 = E0  PIA60415 position=3 = 70  PIA60416 position=4 = 01  PIA60417 position=5 = A7  PIA60418 position=6 = D0  PIA60419 position=7 = 01  PIA60420 position=8 = BD  PIA60421 position=9 = 70  PIA60422 position=10 = 01  PIA60413 position=11 = B4  PIA60414 position=12 = 40 | 2020-120T10:45:30.000Z |
|  | EAS2 MCP RAMP  UniqueID = SSWAEAStest46 | ZIA58832 PIA60218 position=1 = 8E1 | 2020-120T10:46:00.000Z |
|  | EAS2 START SCIENCE  UniqueID = SSWAEAStest47 | ZIA58819 PIA60031 position=1 = MBOX1  PIA60446 position=2 = 0  PIA60447 position=3 = 0  PIA60448 position=4 = 2 | 2020-120T10:47:00.000Z |

2 hours of science

FDIR Test

|  |  |  |  |
| --- | --- | --- | --- |
|  | ENABLE EAS2 FDIR  UniqueID = SSWAEAStest48 | ZIA58063 PIA60452 position=1 = 11  PIA60449 position=2 = EAS2SPWHB\_MI  PIA60449 position=3 = E2\_3V3\_MI  PIA60449 position=4 = E2\_1V5\_MI  PIA60449 position=5 = E2OPTEMPMON  PIA60449 position=6 = E2HVOUTVMON  PIA60449 position=7 = E2MCPVMON  PIA60449 position=8 = E210VAPOSVMON  PIA60449 position=9 = E228VPOSVMON  PIA60449 position=10 = E2HVGENTHERMON  PIA60449 position=11 = E2HVMODTHERMON  PIA60449 position=12 = EAS2MISSACK\_MI | 2020-120T12:47:00.000Z |

30 mins of science

|  |  |  |  |
| --- | --- | --- | --- |
|  | EAS2 STOP SCIENCE  UniqueID = SSWAEAStest49 | ZIA58819 PIA60031 position=1 = MBOX1  PIA60446 position=2 = 0  PIA60447 position=3 = 0  PIA60448 position=4 = 0 | 2020-120T13:20:00.000Z |
|  | EAS2 MCP TO ZERO  UniqueID = SSWAEAStest50 | ZIA58832 PIA60218 position=1 = 0 | 2020-120T13:20:10.000Z |
|  | EAS1 HEATER OFF  UniqueID = SSWAEAStest51 | ZIA58757 PIA60773 position=1 = 00  PIA60774 position=2 = 00  PIA60775 position=3 = 00 | 2020-120T13:21:30.000Z |
|  | EAS2 HEATER OFF  UniqueID = SSWAEAStest52 | ZIA58805 PIA60773 position=1 = 00  PIA60774 position=2 = 00  PIA60775 position=3 = 00 | 2020-120T13:22:00.000Z |
|  | SWITCH OFF EAS1  UniqueID = SSWAEAStest53 | ZIA58756 | 2020-120T13:23:00.000Z |
|  | SWITCH OFF EAS2  UniqueID = SSWAEAStest54 | ZIA58804 | 2020-120T13:23:30.000Z |
|  | STOP EAS1 HK  UniqueID = SSWAEAStest55 | ZIA58051 PIA58050 position=1 = EAS1\_SENS\_HK | 2020-120T13:24:00.000Z |
|  | STOP EAS2 HK  UniqueID = SSWAEAStest56 | ZIA58051 PIA58050 position=1 = EAS2\_SENS\_HK | 2020-120T13:24:10.000Z |

Start PAS

|  |  |  |  |
| --- | --- | --- | --- |
|  | ENABLE PAS HK  UniqueID = SSWAPASon01 | ZIA58050 PIA58050 position=1 = PAS\_SENS\_HK | 2020-120T13:25:00.000Z |
|  | DISABLE PAS FDIR  UniqueID = SSWAPASon02 | ZIA58064 PIA60452 position=1 = 28  PIA60449 position=2 = V\_MON\_C\_MI  PIA60449 position=3 = V\_MON\_L\_MI  PIA60449 position=4 = I\_MON\_C\_MI  PIA60449 position=5 = I\_MON\_L\_MI  PIA60449 position=6 = T\_MON\_C\_MI  PIA60449 position=7 = T\_MON\_L\_MI  PIA60449 position=8 = P24\_VCEMOUT\_MI  PIA60449 position=9 = P5\_VCEMOUT\_MI  PIA60449 position=10 = P12\_VHTOUT\_MI  PIA60449 position=11 = M12\_VHTOUT\_MI  PIA60449 position=12 = P3V\_3\_FPGA\_OMI  PIA60449 position=13 = P1V\_5\_FPGA\_OMI  PIA60449 position=14 = TEMP\_DCDC\_MI  PIA60449 position=15 = TEMP\_FPGA\_MI  PIA60449 position=16 = HK\_IP24V\_CEMMI  PIA60449 position=17 = HK\_IP5V\_CEMMI  PIA60449 position=18 = HK\_IP12V\_HTMI  PIA60449 position=19 = HK\_IM12V\_HTMI  PIA60449 position=20 = HK\_I3V3\_FPGAMI  PIA60449 position=21 = HK\_I1V5\_FPGAMI  PIA60449 position=22 = HK\_IP28V\_PRIMI  PIA60449 position=23 = HK\_MHV\_POSMI  PIA60449 position=24 = HK\_MHV\_NEGMI  PIA60449 position=25 = TEMP\_HVPS\_MI  PIA60449 position=26 = HK\_IP28V\_PRSCI  PIA60449 position=27 = PASampOverCurr  PIA60449 position=28 = PASSPWHB\_MI  PIA60449 position=29 = PASMISSACK\_MI | 2020-120T13:25:10.000Z |
|  | POWER ON PAS  UniqueID = SSWAPASon03 | ZIA58858 | 2020-120T13:25:20.000Z |
|  | MASTER CONTROL REGISTER  UniqueID = SSWAPASon04 | ZIA58863 PIA60343 position=1 = 0000001A | 2020-120T13:27:00.000Z |
|  | ENABLE PAS FDIR  UniqueID = SSWAPASon05 | ZIA58063 PIA60452 position=1 = 3  PIA60449 position=2 = PASSPWHB\_MI  PIA60449 position=3 = PASMISSACK\_MI  PIA60449 position=4 = HK\_IP28V\_PRIMI | 2020-120T13:27:05.000Z |
|  | DISABLE PAS FDIR  UniqueID = SSWAPASon06 | ZIA58064 PIA60452 position=1 = 1  PIA60449 position=2 = HK\_IP28V\_PRIMI | 2020-120T13:27:35.000Z |
|  | ENABLE PAS FDIR  UniqueID = SSWAPASon07 | ZIA58063 PIA60452 position=1 = 1  PIA60449 position=2 = HK\_IP28V\_PRSCI | 2020-120T13:28:05.000Z |
|  | PAS HEATER OFF  UniqueID = SSWAPASon08 | ZIA58947 PIA60848 position=1 = OFF  PIA60849 position=2 = 00 | 2020-120T13:28:20.000Z |
|  | MASTER CONTROL REGISTER  UniqueID = SSWAPASon09 | ZIA58863 PIA60343 position=1 = 0000001E | 2020-120T13:28:30.000Z |
|  | CONF MACRO  UniqueID = SSWAPASon10 | ZIA58853 | 2020-120T13:28:40.000Z |
|  | ENABLE PAS FDIR  UniqueID = SSWAPASon11 | ZIA58063 PIA60452 position=1 = 2  PIA60449 position=2 = P12\_VHTOUT\_MI  PIA60449 position=3 = M12\_VHTOUT\_MI | 2020-120T13:40:00.000Z |
|  | MASTER CONTROL REGISTER  UniqueID = SSWAPASon12 | ZIA58863 PIA60343 position=1 = 0000001F | 2020-120T13:40:30.000Z |
|  | MASTER CONTROL REGISTER  UniqueID = SSWAPASon13 | ZIA58863 PIA60343 position=1 = 00000007 | 2020-120T13:40:40.000Z |
|  | RAMP UP THE HV  UniqueID = SSWAPASon14 | ZIA58856 PIA60791 position=1 = 0000  PIA60790 position=2 = 0570  PIA60792 position=3 = 0029  PIA60793 position=4 = 0019 | 2020-120T13:40:50.000Z |
|  | PREAMPS ON  UniqueID = SSWAPASon15 | ZIA58862 PIA58062 position=1 = ON  PIA58063 position=2 = ON | 2020-120T13:56:00.000Z |
|  | ENABLE PAS FDIR  UniqueID = SSWAPASon16 | ZIA58063 PIA60452 position=1 = 15  PIA60449 position=2 = V\_MON\_C\_MI  PIA60449 position=3 = V\_MON\_L\_MI  PIA60449 position=4 = T\_MON\_C\_MI  PIA60449 position=5 = T\_MON\_L\_MI  PIA60449 position=6 = P24\_VCEMOUT\_MI  PIA60449 position=7 = P5\_VCEMOUT\_MI  PIA60449 position=8 = P3V\_3\_FPGA\_OMI  PIA60449 position=9 = P1V\_5\_FPGA\_OMI  PIA60449 position=10 = TEMP\_DCDC\_MI  PIA60449 position=11 = TEMP\_FPGA\_MI  PIA60449 position=12 = HK\_IP24V\_CEMMI  PIA60449 position=13 = HK\_IP5V\_CEMMI  PIA60449 position=14 = HK\_I3V3\_FPGAMI  PIA60449 position=15 = HK\_I1V5\_FPGAMI  PIA60449 position=16 = TEMP\_HVPS\_MI | 2020-120T13:56:10.000Z |
|  | START CYCLOGRAMS  UniqueID = SSWAPASon17 | ZIA58943 PIA60777 position=1 = PasNc1 | 2020-120T13:57:00.000Z |

1 hour of data

|  |  |  |  |
| --- | --- | --- | --- |
|  | STOP PAS SCIENCE  UniqueID = SSWAPASoff1 | ZIA58944 | 2020-120T15:00:00.000Z |
|  | RAMP DOWN PAS CEM HV  UniqueID = SSWAPASoff2 | ZIA58868 PIA60344 position=1 = 570 | 2020-120T15:00:02.000Z |
|  | RAMP DOWN PAS HV  UniqueID = SSWAPASoff3 | ZIA58857 PIA60790 position=1 = 0000  PIA60791 position=2 = 570  PIA60792 position=3 = 00B2  PIA60793 position=4 = 0006 | 2020-120T15:02:30.000Z |
|  | SWITCH OFF PREAMPS  UniqueID = SSWAPASoff4 | ZIA58862 PIA58062 position=1 = OFF  PIA58063 position=2 = OFF | 2020-120T15:07:00.000Z |
|  | DISABLE FDIR MONITORS  UniqueID = SSWAPASoff5 | ZIA58064 PIA60452 position=1 = 28  PIA60449 position=2 = V\_MON\_C\_MI  PIA60449 position=3 = V\_MON\_L\_MI  PIA60449 position=4 = I\_MON\_C\_MI  PIA60449 position=5 = I\_MON\_L\_MI  PIA60449 position=6 = T\_MON\_C\_MI  PIA60449 position=7 = T\_MON\_L\_MI  PIA60449 position=8 = P24\_VCEMOUT\_MI  PIA60449 position=9 = P5\_VCEMOUT\_MI  PIA60449 position=10 = P12\_VHTOUT\_MI  PIA60449 position=11 = M12\_VHTOUT\_MI  PIA60449 position=12 = P3V\_3\_FPGA\_OMI  PIA60449 position=13 = P1V\_5\_FPGA\_OMI  PIA60449 position=14 = TEMP\_DCDC\_MI  PIA60449 position=15 = TEMP\_FPGA\_MI  PIA60449 position=16 = HK\_IP24V\_CEMMI  PIA60449 position=17 = HK\_IP5V\_CEMMI  PIA60449 position=18 = HK\_IP12V\_HTMI  PIA60449 position=19 = HK\_IM12V\_HTMI  PIA60449 position=20 = HK\_I3V3\_FPGAMI  PIA60449 position=21 = HK\_IP28V\_PRIMI  PIA60449 position=22 = HK\_IP28V\_PRIMI  PIA60449 position=23 = HK\_MHV\_POSMI  PIA60449 position=24 = HK\_MHV\_NEGMI  PIA60449 position=25 = TEMP\_HVPS\_MI  PIA60449 position=26 = HK\_IP28V\_PRSCI  PIA60449 position=27 = PASampOverCurr  PIA60449 position=28 = PASSPWHB\_MI  PIA60449 position=29 = PASMISSACK\_MI | 2020-120T15:07:10.000Z |
|  | POWER OFF  UniqueID = SSWAPASoff6 | ZIA58859 | 2020-120T15:07:20.000Z |

HIS SSD TEST

LEAVE DPU ON

# 30th April. SWA-5 (IA-5)

## MTL PDOR\_SSWA\_SWA\_MTL\_30Apr\_00002.SOL

| **Step N°** | **Commanding Flow** | **FCP ID or PDOR title & contents** | **Comments** |
| --- | --- | --- | --- |
|  | Power DPU on | IA-FCP-011 | Doy 121 09:15  DPU IS LEFT ON. |
|  | Configure the DPU | IA-FCP-030 | Doy 121 09:20 |
|  | Disable EAS1 FDIR | ZIA58064, PIA60452 = 12  PIA60449 = EAS1SPWHB\_MI  PIA60449 = E1\_3V3\_MI  PIA60449 = E1\_1V5\_MI  PIA60449 = E1OPTEMPMON  PIA60449 = E1HVOUTVMON  PIA60449 = E1MCPVMON  PIA60449 = E1GRIDVMON  PIA60449 = E110VAPOSVMON  PIA60449 = E128VPOSVMON  PIA60449 = E1HVGENTHERMON  PIA60449 = E1HVMODTHERMON  PIA60449 = EAS1MISSACK\_MI |  |
|  | Disable EAS2 FDIR | ZIA58064, PIA60452 = 12  PIA60449 = EAS2SPWHB\_MI  PIA60449 = E2\_3V3\_MI  PIA60449 = E2\_1V5\_MI  PIA60449 = E2OPTEMPMON  PIA60449 = E2HVOUTVMON  PIA60449 = E2MCPVMON  PIA60449 = E2GRIDVMON  PIA60449 = E210VAPOSVMON  PIA60449 = E228VPOSVMON  PIA60449 = E2HVGENTHERMON  PIA60449 = E2HVMODTHERMON  PIA60449 = EAS2MISSACK\_MI | 11:00:10 |
|  | Enable EAS1 HK  Power EAS1 on  POST macro on EAS1  IDLE macro on EAS1  Request EAS1 HK | ZIA58050, PIA58050 = EAS1\_SENS\_HK  Wait 00:00:01 (1 second)  ZIA58760  Wait 00:00:05 (5 second)  ZIA58934, PIA60739 = POST  Wait 00:00:05 (5 second)  ZIA58753  Wait 00:00:30 (30 second)  ZIA58782 | 11:01:00 |
|  | RUN macro on EAS1 | ZIA58758  Wait 00:00:20 (20 second) | 11:02:00 |
|  | Enable EAS2 HK  Power EAS2 on  POST macro on EAS2  IDLE macro on EAS2  Request EAS2 HK | ZIA58050, PIA58050 = EAS2\_SENS\_HK  Wait 00:00:01 (1 second)  ZIA58808  Wait 00:00:05 (5 second)  ZIA58936, PIA60740 = POST  Wait 00:00:05 (5 second)  ZIA58801  Wait 00:30:00 (30 second)  ZIA58830 | 11:03:00 |
|  | RUN macro on EAS2 | ZIA58806  Wait 00:00:20 (20 second) | 11:04:00 |
|  | Zero the Deflectors | ZIA58765, PIA60474 = 0x00  PIA60475 = 0x00  PLUS 96 BYTES | 11:05:00 |
|  | Zero the EAS2 Deflectors | ZIA58813, PIA60474 = 0x00  PIA60475 = 0x00  PLUS 96 BYTES | 11:05:10 |
|  | Master Control Register  EAS1 Heater Control | ZIA58776, PIA60423 = 0x00  PIA60424 = 0x40  PIA60425 = 0x60  ZIA58757, PIA60773 = 0x00  PIA60774 = 0x00  PIA60775 = 0xE8 | 11:05:20 |
|  | Master control Register  EAS2 Heater Control | ZIA58824, PIA60423 = 0x00  PIA60424 = 0x40  PIA60425 = 0x60  ZIA58805, PIA60773 = 0x00  PIA60774 = 0x00  PIA60775 = 0xE8 | 11:05:30 |
|  | Set the Hem ratio  Set the Hem Max to 800v  Rebuild Table | ZIA58766, PIA60441 = 0xDE  PIA60442 = 0xB8  PIA60443 = 0x51  ZIA58767, PIA60441 = 67  PIA60442 = 18  PIA60443 = A0  ZIA58771, PIA60031 = MBOX3  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x1 | 11:06:00 |
|  | Set the Hem ratio  Set the Hem Max to 800v  Rebuild Table | ZIA58814, PIA60441 = 0xDE  PIA60442 = 0xB8  PIA60443 = 0x51  ZIA58815, PIA60441 = 67  PIA60442 = 18  PIA60443 = A0  ZIA58819, PIA60031 = MBOX3  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x1 | 11:06:10 |
|  | Adjust the voltage offsets on EAS1 | ZIA58769, PIA60411 = 0x01  PIA60412 = 0x8C  PIA60415 = 0x70  PIA60416 = 0x01  PIA60417 = 0xF6  PIA60418 = 0x00  PIA60419 = 0x01  PIA60420 = 0xC9  PIA60421 = 0xD0  PIA60422 = 0x01  PIA60413 = 0xB6  PIA60414 = 0x00 | 11:06:20 |
|  | Adjust the voltage offsets on EAS2 | ZIA58817, PIA60411 = 0x01  PIA60412 = 0xE0  PIA60415 = 0x70  PIA60416 = 0x01  PIA60417 = 0xA7  PIA60418 = 0xD0  PIA60419 = 0x01  PIA60420 = 0xBD  PIA60421 = 0x70  PIA60422 = 0x01  PIA60413 = 0xB4  PIA60414 = 0x40 | 11:06:30 |
|  | Set the cadence to high | ZIA58728, PIA60096 = HIGH\_CADENCE  PIA60097 = HIGH\_CADENCE  PIA60099 = NOMINAL\_CADENCE  PIA60098 = NOMINAL\_CADENCE | 11:06:40 |
|  | Adjust Thresholds on EAS1 | ZIA58797, PIA60174 = 0x4C80  PIA60185 = 0x4C81  PIA60196 = 0x4C82  PIA60200 = 0x4C83  PIA60201 = 0x4C84  PIA60202 = 0x4C85  PIA60203 = 0x4C86  PIA60204 = 0x4C87  PIA60205 = 0x4C88  PIA60175 = 0x4C89  PIA60176 = 0x4C8A  PIA60177 = 0x4C8B  PIA60178 = 0x4C8C  PIA60179 = 0x4C8D  PIA60180 = 0x4C8E  PIA60181 = 0x4C8F  PIA60182 = 0x4C80  PIA60183 = 0x4C81  PIA60184 = 0x4C82  PIA60186 = 0x4C83  PIA60187 = 0x4C84  PIA60188 = 0x4C85  PIA60189 = 0x4C86  PIA60190 = 0x4C87  PIA60191 = 0x4C88  PIA60192 = 0x4C89  PIA60193 = 0x4C8A  PIA60194 = 0x4C8B  PIA60195 = 0x4C8C  PIA60197 = 0x4C8D  PIA60198 = 0x4C8E  PIA60199 = 0x4C8F | 11:07:00 | |
|  | Set the EAS2 threshold values to 0x4C8 | ZIA58845, PIA60174 = 0x4C80  PIA60185 = 0x4C81  PIA60196 = 0x4C82  PIA60200 = 0x4C83  PIA60201 = 0x4C84  PIA60202 = 0x4C85  PIA60203 = 0x4C86  PIA60204 = 0x4C87  PIA60205 = 0x4C88  PIA60175 = 0x4C89  PIA60176 = 0x4C8A  PIA60177 = 0x4C8B  PIA60178 = 0x4C8C  PIA60179 = 0x4C8D  PIA60180 = 0x4C8E  PIA60181 = 0x4C8F  PIA60182 = 0x4C80  PIA60183 = 0x4C81  PIA60184 = 0x4C82  PIA60186 = 0x4C83  PIA60187 = 0x4C84  PIA60188 = 0x4C85  PIA60189 = 0x4C86  PIA60190 = 0x4C87  PIA60191 = 0x4C88  PIA60192 = 0x4C89  PIA60193 = 0x4C8A  PIA60194 = 0x4C8B  PIA60195 = 0x4C8C  PIA60197 = 0x4C8D  PIA60198 = 0x4C8E  PIA60199 = 0x4C8F | 11:07:20 | |
|  | Ramp the EAS1 MCP | ZIA58784, PIA60218 = 0x8FB | 11:07:40 | |
|  | Start normal mode on EAS1 | ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x2 | 11:08:20 | |
|  | Ramp the EAS2 MCP | ZIA58832, PIA60218 = 0x8E1 | 11:08:30 | |
|  | Start normal mode on EAS2 | ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x2 | 11:09:10 | |

At this point we are OFF the MTL 11:10:00.

## EAS 1&2 Eng Mode 6

|  |  |  |  |
| --- | --- | --- | --- |
| **Step N°** | **Commanding Flow** | **FCP ID or PDOR title & contents** | **Comments** |
|  | Stop normal mode on EAS1  Perform Eng Mode 6 | **PDOR\_SSWA\_EAS1\_EngMode\_6\_00003.SOL**  ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x0  ZIA58792, PIA60457 = 0xFF  PIA60458 = 0x32  PIA60459 = 0x28  PIA60106 = 0x0  PIA60171 = 0xA  PIA60165 = 10 |  |
|  | Stop normal mode on EAS2  Perform Eng Mode 6 | **PDOR\_SSWA\_EAS2\_EngMode\_6\_00003.SOL**  ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x0  ZIA58840, PIA60457 = 0xFF  PIA60458 = 0x32  PIA60459 = 0x28  PIA60106 = 0x0  PIA60171 = 0xA  PIA60165 = 10 |  |

## EAS 2 Zero Sweeps

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Set the Hem Voltage Offsets to zero. | **PDOR\_SSWA\_EAS2\_ZeroHemVoltOffset\_00001.SOL**  ZIA58817, PIA60411 = 0x01  PIA60412 = 0xE0  PIA60415 = 0x70  PIA60416 = 0x01  PIA60417 = 0xA7  PIA60418 = 0xD0  PIA60419 = 0x00  PIA60420 = 0x00  PIA60421 = 0x00  PIA60422 = 0x01  PIA60413 = 0xB4  PIA60414 = 0x40 | |  |
|  | Set the Hem Max to 0v  Rebuild Table | **PDOR\_SSWA\_EAS2\_ZeroHem\_00001.SOL**  ZIA58815, PIA60441 = 0  PIA60442 = 0  PIA60443 = 0  ZIA58819, PIA60031 = MBOX3  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x1 | |  |
|  | Start normal mode on EAS2 | | **PDOR\_SSWA\_EAS2\_NormalMode\_00001.SOL**  ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x2 |  | |

## EAS2 Flight deflectors

|  |  |  |  |
| --- | --- | --- | --- |
|  | Adjust Deflectors on EAS2  Stop Normal Mode on EAS2  Adjust the Deflector Ratios | **PDOR\_SSWA\_EAS2\_Deflectors\_Flight\_00002.SOL**  ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0  ZIA58813, PIA60474 = 0xAD  PIA60475 = 0x0E  PIA60578 = 0x56  PLUS Other Bytes |  |

## EAS2 POST MCP commission

|  |  |  |  |
| --- | --- | --- | --- |
|  | Post EAS2 MCP Commission  Stop normal mode on EAS2  Set the EAS2 MCP to 2695V =  0xAC2  Start normal mode on EAS2 | **PDOR\_SSWA\_EAS2\_Post\_MCP\_Comm\_00002.SOL**  ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0  ZIA58832, PIA60218 = 0xAC2  ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 2 |  |

## EAS 2 Flight Sweeps

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  | Stop normal mode on EAS2  Set the Hem ratio  Set the Hem Max to 800v  Rebuild Table | **PDOR\_SSWA\_EAS2\_FlightSweep\_00002.SOL**  ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x0  ZIA58814, PIA60441 = 0xDE  PIA60442 = 0xB8  PIA60443 = 0x51  ZIA58815, PIA60441 = 67  PIA60442 = 18  PIA60443 = A0  ZIA58819, PIA60031 = MBOX3  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x1 |  |
|  | Adjust the voltage offsets on EAS2 | **PDOR\_SSWA\_EAS2\_FlightVoltOffset\_00002**  ZIA58817, PIA60411 = 0x01  PIA60412 = 0xE0  PIA60415 = 0x70  PIA60416 = 0x01  PIA60417 = 0xA7  PIA60418 = 0xD0  PIA60419 = 0x01  PIA60420 = 0xBD  PIA60421 = 0x70  PIA60422 = 0x01  PIA60413 = 0xB4  PIA60414 = 0x40 |  | |

## EAS2 Start Normal Mode

|  |  |  |  |
| --- | --- | --- | --- |
|  | Start normal mode on EAS2 | **PDOR\_SSWA\_EAS2\_NormalMode\_00001.SOL**  ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x2 |  |

## EAS1 Zero Sweeps

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **PDOR\_SSWA\_EAS1\_ZeroHemOffset\_00001.SOL**  ZIA58769, PIA60411 = 0x01  PIA60412 = 0x8C  PIA60415 = 0x70  PIA60416 = 0x01  PIA60417 = 0xF6  PIA60418 = 0x00  PIA60419 = 0x00  PIA60420 = 0x00  PIA60421 = 0x00  PIA60422 = 0x01  PIA60413 = 0xB6  PIA60414 = 0x00 | THIS PDOR DOESN’T EXIST AT MOC!!!!! |
|  | Set the Hem Max to 0v  Rebuild Table | **PDOR\_SSWA\_EAS1\_ZeroHem\_00001.SOL**  ZIA58767, PIA60441 = 0  PIA60442 = 0  PIA60443 = 0  ZIA58771, PIA60031 = MBOX3  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x1 |  |
|  | Start normal mode on EAS1 | **PDOR\_SSWA\_EAS1\_NormalMode\_00001.SOL**  ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x2 |  |

## EAS1 Flight Sweeps

|  |  |  |  |
| --- | --- | --- | --- |
|  | Stop normal mode on EAS1  Set the Hem ratio  Set the Hem Max to 800v  Rebuild Table | **PDOR\_SSWA\_EAS1\_FlightSweep\_00002.SOL**  ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x0  ZIA58766, PIA60441 = 0xDE  PIA60442 = 0xB8  PIA60443 = 0x51  ZIA58767, PIA60441 = 67  PIA60442 = 18  PIA60443 = A0  ZIA58771, PIA60031 = MBOX3  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x1 |  |

## EAS1 Flight deflectors

|  |  |  |  |
| --- | --- | --- | --- |
|  | Adjust Deflectors on EAS1  Stop Normal Mode on EAS1  Adjust the Deflector Ratios | **PDOR\_SSWA\_EAS1\_Deflectors\_Flight\_00002.SOL**  ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0  ZIA58765, PIA60474 = 0xB0  PIA60475 = 0xC4  PIA60578 = 0x9B  PLUS Other Bytes |  |

## EAS1 POST MCP commission

|  |  |  |  |
| --- | --- | --- | --- |
|  | Post EAS1 MCP Commission  Stop normal mode on EAS1  Set the EAS1 MCP to 2695V =  0xAC2  Start normal mode on EAS1 | **PDOR\_SSWA\_EAS1\_Post\_MCP\_Comm\_00002.SOL**  ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x0  ZIA58784, PIA60218 = 0xAC2  ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x2 |  |

## EAS1 Flight Voltage Offsets

|  |  |  |  |
| --- | --- | --- | --- |
|  | Adjust the voltage offsets on EAS1 | **PDOR\_SSWA\_EAS1\_FlightVoltOffset\_00002.SOL**  ZIA58769, PIA60411 = 0x01  PIA60412 = 0x8C  PIA60415 = 0x70  PIA60416 = 0x01  PIA60417 = 0xF6  PIA60418 = 0x00  PIA60419 = 0x01  PIA60420 = 0xC9  PIA60421 = 0xD0  PIA60422 = 0x01  PIA60413 = 0xB6  PIA60414 = 0x00 |  |

## EAS1 Start Normal Mode

|  |  |  |  |
| --- | --- | --- | --- |
|  | Start normal mode on EAS1 | **PDOR\_SSWA\_EAS1\_NormalMode\_00001.SOL**  ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x2 |  |

**PAUSE. WAIT FOR SWA TO CONTINUE**

## EAS 2 Engineering modes

|  |  |  |  |
| --- | --- | --- | --- |
| **Step N°** | **Commanding Flow** | **FCP ID or PDOR title & contents** | **Comments** |
|  | Perform Eng mode 4 on EAS2  Stop normal mode on EAS2  Eng mode 4 (Threshold Sweep) | **PDOR\_SSWA\_EAS2\_EngMode4\_00005.SOL**  ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0  ZIA58838, PIA60104 = 0x6BC Start Thresh  PIA60103 = 0x4BE End Thresh  PIA60105 = 0x1E Thresh step  PIA60106 = 0xA94 MCP Value  PIA60165 = 0xA MCP wait  PIA60851 = 20 Acq time  PIA60760 = 0xD Hem bin  PIA60761 = 0x8 Def number |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Adjust Thresholds on EAS2  Adjust the Thresholds | **PDOR\_SSWA\_EAS2\_Thresh\_4C8\_00001.SOL**  ZIA58845, PIA60174 = 0x4C80  PIA60185 = 0x4C81  PIA60196 = 0x4C82  Plus other bytes |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Perform Eng mode 3 on EAS2  Stop normal mode on EAS2  Eng mode 3 (Gain Test) | **PDOR\_SSWA\_EAS2\_EngMode3\_00005.SOL**  ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0  ZIA58837, PIA60101 = 0x869  PIA60100 = 0xA94  PIA60102 = 0x1E Step MCP  PIA60437 = 0xA 1st ramp time  PIA60444 = 0x1 Inter ramp time  PIA60165 = 40 Acq time  PIA60760 = 0xD Hem bin  PIA60761 = 0x8 Def number  PIA60762 = SWEEP\_MACRO ctrl |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Stop normal mode on EAS1  Reset the MCP to AC2 | **PDOR\_SSWA\_EAS2\_FlightMCP\_00001.SOL**  ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x0  ZIA58832, PIA60218 = 0xAC2 |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **PDOR\_SSWA\_EAS2\_ZeroVoltOffset\_00001.SOL**  ZIA58817, PIA60411 = 0x00  PIA60412 = 0x00  PIA60415 = 0x00  PIA60416 = 0x00  PIA60417 = 0x00  PIA60418 = 0x00  PIA60419 = 0x00  PIA60420 = 0x00  PIA60421 = 0x00  PIA60422 = 0x00  PIA60413 = 0x00  PIA60414 = 0x00 |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Set the Hem Max to 0v  Rebuild Table | **PDOR\_SSWA\_EAS2\_ZeroHem\_00001.SOL**  ZIA58815, PIA60441 = 0  PIA60442 = 0  PIA60443 = 0  ZIA58819, PIA60031 = MBOX3  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x1 |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Eng mode 5 (Threshold Sweep)  Stop Science  Start Eng Mode 5 | **PDOR\_SSWA\_EAS2\_HV\_EngMode\_5\_00002.SOL**  ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0  Wait 00:00:01 (1 second)  ZIA58839, PIA60454 = 0x32 PA1 stim  PIA60455 = 0x32 PA2 stim  PIA60040 = 0x500 Start Thresh  PIA60039 = 0x47E End Thresh  PIA60041 = 0x4 Thresh step  PIA60106 = 0xAC2 MCP value  PIA60171 = 1 MCP wait  PIA60165 = 2 Acq time  Wait 00:01:10 (70 second) |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Perform Eng mode 4 on EAS2  Stop normal mode on EAS2  Eng mode 4 (Threshold Sweep) | **PDOR\_SSWA\_EAS2\_EngMode4\_00005.SOL**  ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0  ZIA58838, PIA60104 = 0x6BC Start Thresh  PIA60103 = 0x4BE End Thresh  PIA60105 = 0x1E Thresh step  PIA60106 = 0xA94 MCP Value  PIA60165 = 0xA MCP wait  PIA60851 = 20 Acq time  PIA60760 = 0xD Hem bin  PIA60761 = 0x8 Def number |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Perform Eng mode 3 on EAS2  Stop normal mode on EAS2  Eng mode 3 (Gain Test) | **PDOR\_SSWA\_EAS2\_EngMode3\_00005.SOL**  ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0  ZIA58837, PIA60101 = 0x869  PIA60100 = 0xA94  PIA60102 = 0x1E Step MCP  PIA60437 = 0xA 1st ramp time  PIA60444 = 0x1 Inter ramp time  PIA60165 = 40 Acq time  PIA60760 = 0xD Hem bin  PIA60761 = 0x8 Def number  PIA60762 = SWEEP\_MACRO ctrl |  |

## EAS 2 Reset Sweeps

|  |  |  |  |
| --- | --- | --- | --- |
|  | Stop normal mode on EAS2  Set the Hem Ratio  Set the Hem Max to 800v  Rebuild Table | **PDOR\_SSWA\_EAS2\_FlightSweep\_00002.SOL**  ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x0  ZIA58814, PIA60441 = 0xDE  PIA60442 = 0xB8  PIA60443 = 0x51  ZIA58815, PIA60441 = 67  PIA60442 = 18  PIA60443 = A0  ZIA58819, PIA60031 = MBOX3  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x1 |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Adjust Deflectors on EAS2  Stop Normal Mode on EAS2  Adjust the Deflector Ratios | **PDOR\_SSWA\_EAS2\_Deflectors\_Flight\_00002.SOL**  ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0  ZIA58813, PIA60474 = 0xAD  PIA60475 = 0x0E  PIA60578 = 0x56  PLUS Other Bytes |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Adjust Thresholds on EAS2  Adjust the Thresholds | **PDOR\_SSWA\_EAS2\_Thresh\_4C8\_00001.SOL**  ZIA58845, PIA60174 = 0x4C80  PIA60185 = 0x4C81  Plus other bytes |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Adjust the voltage offsets on EAS2 | **PDOR\_SSWA\_EAS2\_FlightVoltOffset\_00002.SOL**  ZIA58817, PIA60411 = 0x01  PIA60412 = 0xE0  PIA60415 = 0x70  PIA60416 = 0x01  PIA60417 = 0xA7  PIA60418 = 0xD0  PIA60419 = 0x01  PIA60420 = 0xBD  PIA60421 = 0x70  PIA60422 = 0x01  PIA60413 = 0xB4  PIA60414 = 0x40 |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Start normal mode on EAS2 | **PDOR\_SSWA\_EAS2\_NormalMode\_00001.SOL**  ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x2 |  |

**PAUSE. WAIT FOR SWA TO CONTINUE**

## EAS 1 Engineering modes

|  |  |  |  |
| --- | --- | --- | --- |
| **Step N°** | **Commanding Flow** | **FCP ID or PDOR title & contents** | **Comments** |
|  | Perform Eng mode 4 on EAS1  Stop normal mode on EAS1  Eng mode 4 (Threshold Sweep) | **PDOR\_SSWA\_EAS1\_EngMode4\_00005.SOL**  ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0  ZIA58790, PIA60104 = 0x6BC Start Thresh  PIA60103 = 0x4BE End Thresh  PIA60105 = 0x1E Thresh step  PIA60106 = 0xA94 MCP Value  PIA60165 = 0xA MCP wait  PIA60851 = 20 Acq time  PIA60760 = 0x13 Hem bin  PIA60761 = 0x8 Def number |  |
|  | Adjust Thresholds on EAS1  Adjust the Thresholds | **PDOR\_SSWA\_EAS1\_Thresh\_4C8\_00001.SOL**  ZIA58797, PIA60174 = 0x4C80  PIA60185 = 0x4C81  Plus other bytes |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Perform Eng mode 3 on EAS1  Stop normal mode on EAS1  Eng mode 3 (Gain Test) | **PDOR\_SSWA\_EAS1\_EngMode3\_00005.SOL**  ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x0  ZIA58789, PIA60101 = 0x869  PIA60100 = 0xA53  PIA60102 = 0x1E Step MCP  PIA60437 = 0xA 1st ramp time  PIA60444 = 0x1 Inter ramp time  PIA60165 = 40 Acq time  PIA60760 = 0xD Hem bin  PIA60761 = 0x8 Def number  PIA60762 = SWEEP\_MACRO ctrl |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Stop normal mode on EAS1  Reset the MCP to AC2 | **PDOR\_SSWA\_EAS1\_FlightMCP\_00001.SOL**  ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x0  ZIA58784, PIA60218 = 0xAC2 |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **PDOR\_SSWA\_EAS1\_ZeroVoltOffset\_00002.SOL**  ZIA58769, PIA60411 = 0x00  PIA60412 = 0x00  PIA60415 = 0x00  PIA60416 = 0x00  PIA60417 = 0x00  PIA60418 = 0x00  PIA60419 = 0x00  PIA60420 = 0x00  PIA60421 = 0x00  PIA60422 = 0x00  PIA60413 = 0x00  PIA60414 = 0x00 |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Set the Hem Max to 0v  Rebuild Table | **PDOR\_SSWA\_EAS1\_ZeroHem\_00001.SOL**  ZIA58767, PIA60441 = 0  PIA60442 = 0  PIA60443 = 0  ZIA58771, PIA60031 = MBOX3  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x1 |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Eng mode 5 (Threshold Sweep)  Stop Science  Start Eng Mode 5 | **PDOR\_SSWA\_EAS1\_HV\_EngMode\_5\_00002.SOL**  ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0  Wait 00:00:01 (1 second)  ZIA58791, PIA60454 = 0x32 PA1 stim  PIA60455 = 0x32 PA2 stim  PIA60040 = 0x500 Start Thresh  PIA60039 = 0x47E End Thresh  PIA60041 = 0x4 Thresh step  PIA60106 = 0xAC2 MCP value  PIA60171 = 1 MCP wait  PIA60165 = 2 Acq time  Wait 00:01:10 (70 second) |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Perform Eng mode 4 on EAS1  Stop normal mode on EAS1  Eng mode 4 (Threshold Sweep) | **PDOR\_SSWA\_EAS1\_EngMode4\_00005.SOL**  ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0  ZIA58790, PIA60104 = 0x6BC Start Thresh  PIA60103 = 0x4BE End Thresh  PIA60105 = 0x1E Thresh step  PIA60106 = 0xA94 MCP Value  PIA60165 = 0xA MCP wait  PIA60851 = 20 Acq time  PIA60760 = 0xD Hem bin  PIA60761 = 0x8 Def number |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Perform Eng mode 3 on EAS1  Stop normal mode on EAS1  Eng mode 3 (Gain Test) | **PDOR\_SSWA\_EAS1\_EngMode3\_00005.SOL**  ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x0  ZIA58789, PIA60101 = 0x869  PIA60100 = 0xA53  PIA60102 = 0x1E Step MCP  PIA60437 = 0xA 1st ramp time  PIA60444 = 0x1 Inter ramp time  PIA60165 = 40 Acq time  PIA60760 = 0xD Hem bin  PIA60761 = 0x8 Def number  PIA60762 = SWEEP\_MACRO ctrl |  |

## EAS 1 Reset Sweeps

|  |  |  |  |
| --- | --- | --- | --- |
|  | Stop normal mode on EAS1  Set the Hem Ratio  Set the Hem Max to 800v  Rebuild Table | **PDOR\_SSWA\_EAS1\_FlightSweep\_00002.SOL**  ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x0  ZIA58766, PIA60469 = DE  PIA60470 = B8  PIA60471 = 53  ZIA58767, PIA60441 = 67  PIA60442 = 18  PIA60443 = A0  ZIA58771, PIA60031 = MBOX3  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x1 |  |
|  | Adjust Deflectors on EAS1  Stop Normal Mode on EAS1  Adjust the Deflector Ratios | **PDOR\_SSWA\_EAS1\_Deflectors\_Flight\_00002.SOL**  ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0  ZIA58765, PIA60474 = 0xB0  PIA60475 = 0xC4  PIA60578 = 0x9B  PLUS Other Bytes |  |
|  | Adjust Thresholds on EAS1  Adjust the Thresholds | **PDOR\_SSWA\_EAS1\_Thresh\_4C8\_00001.SOL**  ZIA58797, PIA60174 = 0x4C80  PIA60185 = 0x4C81  Plus other bytes |  |
|  | Adjust the voltage offsets on EAS1 | **PDOR\_SSWA\_EAS1\_FlightVoltOffset\_00002.SOL**  ZIA58769, PIA60411 = 0x01  PIA60412 = 0x8C  PIA60415 = 0x70  PIA60416 = 0x01  PIA60417 = 0xF6  PIA60418 = 0x00  PIA60419 = 0x01  PIA60420 = 0xC9  PIA60421 = 0xD0  PIA60422 = 0x01  PIA60413 = 0xB6  PIA60414 = 0x00 |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Start normal mode on EAS1 | **PDOR\_SSWA\_EAS1\_NormalMode\_00001.SOL**  ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x2 |  |

**PAUSE. WAIT FOR SWA TO CONTINUE**

## EAS Flight Like Gain Test

|  |  |  |  |
| --- | --- | --- | --- |
|  | Perform Eng mode 3 on EAS1  Stop normal mode on EAS1  Stop normal mode on EAS2  Sweep Eng mode 3 (Gain Test)  On EAS1  Fixed Eng mode 3 (Gain Test)  On EAS2  Wait  Fixed Eng mode 3 (Gain Test)  On EAS1  Sweep Eng mode 3 (Gain Test)  On EAS2  Wait | **PDOR\_SSWA\_EAS\_GainTest\_00003.SOL**  ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x0  ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0  ZIA58789, PIA60101 = 0x869  PIA60100 = 0xA53  PIA60102 = 0x1E Step MCP  PIA60437 = 0xA 1st ramp time  PIA60444 = 1 Inter ramp time  PIA60165 = 40 Acq time  PIA60760 = 0xD Hem bin  PIA60761 = 0x8 Def number  PIA60762 = SWEEP\_MACRO ctrl  No time between these.  ZIA58837, PIA60101 = 0x869  PIA60100 = 0xA53  PIA60102 = 0x1E Step MCP  PIA60437 = 0xA 1st ramp time  PIA60444 = 1 Inter ramp time  PIA60165 = 40 Acq time  PIA60760 = 0xD Hem bin  PIA60761 = 0x8 Def number  PIA60762 = FIXED\_MACRO ctrl  Wait 20\*steps +2  ZIA58789, PIA60101 = 0x869  PIA60100 = 0xA53  PIA60102 = 0x1E Step MCP  PIA60437 = 10 1st ramp time  PIA60444 = 1 Inter ramp time  PIA60165 = 40 Acq time  PIA60760 = 0xD Hem bin  PIA60761 = 0x8 Def number  PIA60762 = FIXED\_MACRO ctrl  No time between these.  ZIA58837, PIA60101 = 0x869  PIA60100 = 0xA53  PIA60102 = 0x1E Step MCP  PIA60437 = 10 1st ramp time  PIA60444 = 1 Inter ramp time  PIA60165 = 40 Acq time  PIA60760 = 0xD Hem bin  PIA60761 = 0x8 Def number  PIA60762 = SWEEP\_MACRO ctrl  Wait 20 x steps +2 |  |

## EAS Reset MCP

|  |  |  |  |
| --- | --- | --- | --- |
|  | Stop normal mode on EAS1  Reset the MCP to AC2 | **PDOR\_SSWA\_EAS1\_FlightMCP\_00002.SOL**  ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x0  ZIA58784, PIA60218 = 0xA94 |  |
|  | Stop normal mode on EAS2  Reset the MCP to AC2 | **PDOR\_SSWA\_EAS2\_FlightMCP\_00002.SOL**  ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x0  ZIA58832, PIA60218 = 0xA94 |  |

## EAS Start Normal Mode

|  |  |  |  |
| --- | --- | --- | --- |
|  | Start normal mode on EAS1 | **PDOR\_SSWA\_EAS1\_NormalMode\_00001.SOL**  ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x2 |  |
|  | Start normal mode on EAS2 | **PDOR\_SSWA\_EAS2\_NormalMode\_00001.SOL**  ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x2 |  |

RAMP MCP To Zero

## EAS 1&2 Eng Mode 7

|  |  |  |  |
| --- | --- | --- | --- |
|  | Eng mode 7 (HV Sweep TEST)  Stop Science  Start Eng Mode 7 | **PDOR\_SSWA\_EAS1\_EngMode\_7\_00001.SOL**  ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0  ZIA58793  Wait 00:02:00 (120 second) |  |
|  | Eng mode 7 (HV Sweep TEST)  Stop Science  Start Eng Mode 7 | **PDOR\_SSWA\_EAS2\_EngMode\_7\_00001.SOL**  ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0  ZIA58841  Wait 00:02:00 (120 second) |  |

## EAS FDIR Commission

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **PDOR\_SSWA\_EAS1\_ENABLE\_FDIR\_00001.SOL**  ZIA58063, PIA60452 = 12  PIA60449 = EAS1SPWHB\_MI  PIA60449 = E1\_3V3\_MI  PIA60449 = E1\_1V5\_MI  PIA60449 = E1OPTEMPMON  PIA60449 = E1HVOUTVMON  PIA60449 = E1MCPVMON  PIA60449 = E1GRIDVMON  PIA60449 = E110VAPOSVMON  PIA60449 = E128VPOSVMON  PIA60449 = E1HVGENTHERMON  PIA60449 = E1HVMODTHERMON  PIA60449 = EAS1MISSACK\_MI |  |
|  |  | **PDOR\_SSWA\_EAS2\_ENABLE\_FDIR\_00001.SOL**  ZIA58063, PIA60452 = 12  PIA60449 = EAS2SPWHB\_MI  PIA60449 = E2\_3V3\_MI  PIA60449 = E2\_1V5\_MI  PIA60449 = E2OPTEMPMON  PIA60449 = E2HVOUTVMON  PIA60449 = E2MCPVMON  PIA60449 = E2GRIDVMON  PIA60449 = E210VAPOSVMON  PIA60449 = E228VPOSVMON  PIA60449 = E2HVGENTHERMON  PIA60449 = E2HVMODTHERMON  PIA60449 = EAS2MISSACK\_MI |  |

## EAS Reset MCP

|  |  |  |  |
| --- | --- | --- | --- |
|  | Stop normal mode on EAS1  Reset the MCP to AC2 | **PDOR\_SSWA\_EAS1\_FlightMCP\_00002.SOL**  ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x0  ZIA58784, PIA60218 = 0xA94 |  |
|  | Stop normal mode on EAS2  Reset the MCP to AC2 | **PDOR\_SSWA\_EAS2\_FlightMCP\_00002.SOL**  ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x0  ZIA58832, PIA60218 = 0xA94 |  |

## EAS Start Normal Mode

|  |  |  |  |
| --- | --- | --- | --- |
|  | Start normal mode on EAS1 | **PDOR\_SSWA\_EAS1\_NormalMode\_00001.SOL**  ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x2 |  |
|  | Start normal mode on EAS2 | **PDOR\_SSWA\_EAS2\_NormalMode\_00001.SOL**  ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x2 |  |

## EAS Configure heater

| **Step N°** | **Commanding Flow** | **FCP ID or PDOR title & contents** | **Comments** |
| --- | --- | --- | --- |
|  | Turn the manual heater on for EAS1  Master Control Register  Heater Control | **PDOR\_SSWA\_EAS1\_Full\_Heater\_00001.SOL**  ZIA58776, PIA60423 = 0x00  PIA60424 = 0x40  PIA60425 = 0x60  ZIA58757, PIA60773 = 0x00  PIA60774 = 0x01  PIA60775 = 0x60 | Control EAS heaters to max  0x160 |
|  | Turn the manual heater on for EAS2  Master control Register  Heater Control | **PDOR\_SSWA\_EAS2\_Full\_Heater\_00001.SOL**  ZIA58824, PIA60423 = 0x00  PIA60424 = 0x40  PIA60425 = 0x60  ZIA58805, PIA60773 = 0x00  PIA60774 = 0x01  PIA60775 = 0x60 | Control EAS1 heaters to max  0x160 |

## MTL PDOR\_SSWA\_SWA\_MTL\_30Apr\_00001.SOL

Before the activity starts, the end of day commanding is loaded onto the MTL. This is shown here as it is unknown at this point where this activity will end. Wherever the end is, the activity will be halted, EAS powered down. Then the following day will power up and continue where this activity ended.

| **Step N°** | **Commanding Flow** | **FCP ID or PDOR title & contents** | **Comments** | |
| --- | --- | --- | --- | --- |
|  | EAS1 Stop Science  EAS1 Ramp MCP to zero  EAS2 Stop Science  EAS2 Ramp MCP to zero  Turn EAS1 heater off  Turn EAS2 heater off  EAS1 Switch Off  EAS2 Switch Off  Stop EAS1 HK  Stop EAS2 HK  Power down DPU | ZIA58771, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x0  ZIA58784, PIA60218 = 0  ZIA58819, PIA60031 = MBOX1  PIA60446 = 0  PIA60447 = 0  PIA60448 = 0x0  ZIA58832, PIA60218 = 0  ZIA58757, PIA60773 = 0  PIA60774 = 0  PIA60775 = 0  ZIA58805, PIA60773 = 0  PIA60774 = 0  PIA60775 = 0  ZIA58756  ZIA8804  ZIA58051, PIA58050 = EAS1\_SENS\_HK  ZIA58051, PIA58050 = EAS2\_SENS\_HK  IA-FCP-002 | | 19:20:30  19:21:00  19:21:30  19:22:00  19:23:00  19:24:00  19:25:00  19:25:30  19:26:00  19:26:01  19:27:00 |

# 5th May. SWA-4 (IA-4) PAS

# 6th May. SWA-4 (IA-4) PAS

# 7th May. SWA-6 (IA-6) SWA

# 8th May. SWA-6 (IA-6) SWA

This section will test the SWA suite in Normal mode. It will then test the SWA Burst mode. The various cadences of the SWA sensors are also tested.

## MTL PDOR\_SSWA\_SWA\_MTL\_8th\_00001.SOL

| **Step N°** | **Commanding Flow** | **FCP ID or PDOR title & contents** | **Comments** |
| --- | --- | --- | --- |
|  | Power DPU on into OPS | **PDOR\_SSWA\_DPU\_Off2Ops\_00001.SOL** | 06:22:00 |
|  | Power up & configure HIS with ramped-up High Voltage ready to sweep. | **PDOR\_SSWA\_HIS\_PowerUpConfig\_00001.SOL** | 06:30 |
|  | Wait 1 hour 22 mins | Wait 01:22:00 |  |
|  | Power up & configure PAS in No science. | **PDOR\_SSWA\_PAS\_Config4Flight\_00001.SOL** |  |
|  | Wait 0 hour 30 mins | Wait 00:30:00 |  |
|  | Power up & configure PAS in No science. | **PDOR\_SSWA\_EAS1\_Config4Flight\_00001.SOL** |  |
|  | Wait 0 hour 30 mins | Wait 00:30:00 |  |
|  | Power up & configure PAS in No science. | **PDOR\_SSWA\_EAS2\_Config4Flight\_00001.SOL** |  |
|  | Wait 0 hour 30 mins | Wait 00:30:00 |  |

At this point all SWA sensors are powered on and configured ready for science.

## SWA Normal mode

|  |  |  |  |
| --- | --- | --- | --- |
| **Step N°** | **Commanding Flow** | **FCP ID or PDOR title & contents** | **Comments** |
|  | Puts HIS into NM | **PDOR\_SSWA\_HIS\_NORMSCI\_00001.SOL** |  |
|  |  | Wait 00:10:00 (600 seconds) |  |
|  | Put PAS into NM | **PDOR\_SSWA\_PAS\_NM\_00001.SOL** |  |
|  |  | Wait 00:10:00 (600 seconds) |  |
|  | HIS to HVSTBY | **PDOR\_SSWA\_HIS\_HVSTBY\_00001.SOL** |  |
|  | EAS 1&2 into NM | **PDOR\_SSWA\_EAS1\_NormalMode\_00001.SOL**  **PDOR\_SSWA\_EAS2\_NormalMode\_00001.SOL** |  |
|  |  | Wait 00:10:00 (600 seconds) |  |
|  | PAS into No Science | **PDOR\_SSWA\_PAS\_NoScience\_00001.SOL** |  |
|  | Puts HIS into NM | **PDOR\_SSWA\_HIS\_NORMSCI\_00001.SOL** |  |
|  |  | Wait 00:10:00 (600 seconds) |  |
|  |  | **PDOR\_SSWA\_PAS\_NM\_00001.SOL** |  |
|  |  | Wait 00:10:00 (600 seconds) |  |
|  | Enable Compression | IA-FCP-101 |  |

## SWA Burst mode

|  |  |  |  |
| --- | --- | --- | --- |
| **Step N°** | **Commanding Flow** | **FCP ID or PDOR title & contents** | **Comments** |
|  | Test Burst Mode  All sensors into BM for 5 mins  5m = 300s / 8 = 2400  PAS only into BM for 5 mins  5m = 300s / 8 = 2400 | **PDOR\_SSWA\_Suite\_Comm\_BM\_00001.SOL**  Wait 00:10:00 (600 seconds)  ZIA58726, PIA60157 = 2400  PIA60158 = 0  PIA60159 = 2400  PIA60160 = 0  PIA60163 = 2400  PIA60164 = 0  PIA60170 = DYNAMIC  PIA60161 = 2400  PIA60162 = 0  Wait 00:20:00 (1200 seconds)  ZIA58726, PIA60157 = 0  PIA60158 = 0  PIA60159 = 0  PIA60160 = 0  PIA60163 = 2400  PIA60164 = 0  PIA60170 = DYNAMIC  PIA60161 = 0  PIA60162 = 0  Wait 00:20:00 (1200 seconds) |  |

All sensors return to Normal Mode.

## SWA Cadence test

|  |  |  |  |
| --- | --- | --- | --- |
| **Step N°** | **Commanding Flow** | **FCP ID or PDOR title & contents** | **Comments** |
|  | Test SWA Cadences  Decrease All SWA cadence  Increase EAS cadence  All SWA at nominal cadence | **PDOR\_SSWA\_Suite\_Comm\_Cadence\_00002.SOL**  ZIA58728, PIA60096 = 2  PIA60097 = 2  PIA60099 = 2  PIA60098 = 2  Wait 00:10:00 (600 seconds)  ZIA58728, PIA60096 = 0  PIA60097 = 0  PIA60099 = 1  PIA60098 = 1  Wait 00:10:00 (600 seconds)  ZIA58728, PIA60096 = 1  PIA60097 = 1  PIA60099 = 1  PIA60098 = 1  Wait 00:10:00 (600 seconds) |  |
|  | Enter Low Cadence Mode  Select Product Configuration Table 3 for Max Res  VDF  Select "SWA\_HIS\_LOW\_1TENTH" PHA  Select "SWA\_HIS\_LOW\_1TENTH" VDF  Select "SWA\_HIS\_LOW\_QUARTER" PHA  Select "SWA\_HIS\_LOW\_QUARTER" VDF  Select "SWA\_HIS\_LOW\_HALF" PHA  Select "SWA\_HIS\_LOW\_HALF" VDF  Select "SWA\_HIS\_LOW\_2THIRDS" PHA  Select "SWA\_HIS\_LOW\_2THIRDS" VDF  Enter Normal Cadence Mode  Select "SWA\_HIS\_NORMAL\_5X" PHA  Select "SWA\_HIS\_NORMAL\_5X" VDF  Select "SWA\_HIS\_NORMAL\_3X" PHA  Select "SWA\_HIS\_NORMAL\_3X" VDF  Select "SWA\_HIS\_NORMAL\_2X" PHA  Select "SWA\_HIS\_NORMAL\_2X" VDF  Select Product Configuration Table 0 for Half  Res VDF  Select "SWA\_HIS\_NORMAL" PHA  Select "SWA\_HIS\_NORMAL" VDF  Select Burst PHA  Select Burst PHA  Select Burst VDF  Select Burst VDF  Setup DPU for 5-minute HIS core burst  Setup DPU for 5-minute HIS optional burst  Command NOP to hold wait time | **PDOR\_SSWA\_HIS\_DATA\_RATE\_CADENCES\_00002.SOL**  Wait 0:00:01 (1 seconds)  ZIA58913, PIA60001 = 8  Wait 0:01:00 (60 seconds)  ZIA58919, PIA60356 = PR\_CONF\_TAB\_NO  PIA60352 = 3  Wait 0:00:01 (1 seconds)  ZIA58919, PIA60356 = PHA\_MAX\_NORMAL  PIA60352 = 5654  Wait 0:00:01 (1 seconds)  ZIA58919, PIA60356 = VDF\_EN\_NORM  PIA60352 = 0  Wait 0:22:00 (1320 seconds)  ZIA58919, PIA60356 = PHA\_MAX\_NORMAL  PIA60352 = 8928  Wait 0:00:01 (1 seconds)  ZIA58919, PIA60356 = VDF\_EN\_NORM  PIA60352 = 1  Wait 0:22:00 (1320 seconds)  ZIA58919, PIA60356 = PHA\_MAX\_NORMAL  PIA60352 = 11904  Wait 0:00:01 (1 seconds)  ZIA58919, PIA60356 = VDF\_EN\_NORM  PIA60352 = 1  Wait 0:22:00 (1320 seconds)  ZIA58919, PIA60356 = PHA\_MAX\_NORMAL  PIA60352 = 23808  Wait 0:00:01 (1 seconds)  ZIA58919, PIA60356 = VDF\_EN\_NORM  PIA60352 = 7  Wait 0:22:00 (1320 seconds)  ZIA58913, PIA60001 = 15  Wait 0:00:10 (10 seconds)  ZIA58919, PIA60356 = PHA\_MAX\_NORMAL  PIA60352 = 11904  Wait 0:00:01 (1 seconds)  ZIA58919, PIA60356 = VDF\_EN\_NORM  PIA60352 = 7  Wait 0:17:00 (1020 seconds)  ZIA58919, PIA60356 = PHA\_MAX\_NORMAL  PIA60352 = 13094  Wait 0:00:01 (1 seconds)  ZIA58919, PIA60356 = VDF\_EN\_NORM  PIA60352 = 1  Wait 0:12:00 (720 seconds)  ZIA58919, PIA60356 = PHA\_MAX\_NORMAL  PIA60352 = 5654  Wait 0:00:01 (1 seconds)  ZIA58919, PIA60356 = VDF\_EN\_NORM  PIA60352 = 1  Wait 0:12:00 (720 seconds)  ZIA58919, PIA60356 = PR\_CONF\_TAB\_NO  PIA60352 = 0  Wait 0:00:01 (1 seconds)  ZIA58919, PIA60356 = PHA\_MAX\_NORMAL  PIA60352 = 5357  Wait 0:00:01 (1 seconds)  ZIA58919, PIA60356 = VDF\_EN\_NORM  PIA60352 = 1  Wait 0:12:00 (720 seconds)  ZIA58919, PIA60356 = PHA\_MAX\_BURST\_1  PIA60352 = 4000  Wait 0:00:01 (1 seconds)  ZIA58919, PIA60356 = PHA\_TLM\_MAX\_B2  PIA60352 = 4000  Wait 0:00:01 (1 seconds)  ZIA58919, PIA60356 = VDF\_EN\_BURST\_1  PIA60352 = 0x3F  Wait 0:00:01 (1 seconds)  ZIA58919, PIA60356 = VDF\_EN\_B2  PIA60352 = 0x3F  Wait 0:00:01 (1 seconds)  ZIA58726, PIA60157 = 0  PIA60158 = 0  PIA60159 = 0  PIA60160 = 0  PIA60163 = 0  PIA60164 = 0  PIA60170 = DYNAMIC  PIA60161 = 2400  PIA60162 = 0  Wait 0:10:00 (600 seconds)  ZIA58726, PIA60157 = 0  PIA60158 = 0  PIA60159 = 0  PIA60160 = 0  PIA60163 = 0  PIA60164 = 0  PIA60170 = DYNAMIC  PIA60161 = 0  PIA60162 = 2400  Wait 0:10:00 (600 seconds)  ZIA58915 |  |

# SWA Commission conclusion

At this point, SWA is fully commissioned.